From c0b70d0e23e953cdaa5de9ee0a7d41629809c6f0 Mon Sep 17 00:00:00 2001
From: "K. Y. Srinivasan" <kys@microsoft.com>
Date: Mon, 14 Dec 2015 16:01:43 -0800
Subject: [PATCH 17/44] Drivers: hv: vmbus: Use uuid_le type consistently

Consistently use uuid_le type in the Hyper-V driver code.

Signed-off-by: K. Y. Srinivasan <kys@microsoft.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
(cherry picked from commit af3ff643ea91ba64dd8d0b1cbed54d44512f96cd)
---
 drivers/hv/channel_mgmt.c       |  2 +-
 drivers/hv/vmbus_drv.c          | 10 ++---
 include/linux/hyperv.h          | 92 ++++++++++++++---------------------------
 include/linux/mod_devicetable.h |  2 +-
 scripts/mod/file2alias.c        |  2 +-
 5 files changed, 40 insertions(+), 68 deletions(-)

diff --git a/drivers/hv/channel_mgmt.c b/drivers/hv/channel_mgmt.c
index a562318b856b..339277b76468 100644
--- a/drivers/hv/channel_mgmt.c
+++ b/drivers/hv/channel_mgmt.c
@@ -409,7 +409,7 @@ static void init_vp_index(struct vmbus_channel *channel, const uuid_le *type_gui
 	struct cpumask *alloced_mask;
 
 	for (i = IDE; i < MAX_PERF_CHN; i++) {
-		if (!memcmp(type_guid->b, hp_devs[i].guid,
+		if (!memcmp(type_guid->b, &hp_devs[i].guid,
 				 sizeof(uuid_le))) {
 			perf_chn = true;
 			break;
diff --git a/drivers/hv/vmbus_drv.c b/drivers/hv/vmbus_drv.c
index 802dcb409030..f1fbb6b98f5c 100644
--- a/drivers/hv/vmbus_drv.c
+++ b/drivers/hv/vmbus_drv.c
@@ -533,7 +533,7 @@ static int vmbus_uevent(struct device *device, struct kobj_uevent_env *env)
 
 static const uuid_le null_guid;
 
-static inline bool is_null_guid(const __u8 *guid)
+static inline bool is_null_guid(const uuid_le *guid)
 {
 	if (memcmp(guid, &null_guid, sizeof(uuid_le)))
 		return false;
@@ -546,9 +546,9 @@ static inline bool is_null_guid(const __u8 *guid)
  */
 static const struct hv_vmbus_device_id *hv_vmbus_get_id(
 					const struct hv_vmbus_device_id *id,
-					const __u8 *guid)
+					const uuid_le *guid)
 {
-	for (; !is_null_guid(id->guid); id++)
+	for (; !is_null_guid(&id->guid); id++)
 		if (!memcmp(&id->guid, guid, sizeof(uuid_le)))
 			return id;
 
@@ -565,7 +565,7 @@ static int vmbus_match(struct device *device, struct device_driver *driver)
 	struct hv_driver *drv = drv_to_hv_drv(driver);
 	struct hv_device *hv_dev = device_to_hv_device(device);
 
-	if (hv_vmbus_get_id(drv->id_table, hv_dev->dev_type.b))
+	if (hv_vmbus_get_id(drv->id_table, &hv_dev->dev_type))
 		return 1;
 
 	return 0;
@@ -582,7 +582,7 @@ static int vmbus_probe(struct device *child_device)
 	struct hv_device *dev = device_to_hv_device(child_device);
 	const struct hv_vmbus_device_id *dev_id;
 
-	dev_id = hv_vmbus_get_id(drv->id_table, dev->dev_type.b);
+	dev_id = hv_vmbus_get_id(drv->id_table, &dev->dev_type);
 	if (drv->probe) {
 		ret = drv->probe(dev, dev_id);
 		if (ret != 0)
diff --git a/include/linux/hyperv.h b/include/linux/hyperv.h
index 10dda1e3b560..4712d7d07b8c 100644
--- a/include/linux/hyperv.h
+++ b/include/linux/hyperv.h
@@ -1012,6 +1012,8 @@ int vmbus_allocate_mmio(struct resource **new, struct hv_device *device_obj,
 	.guid = { g0, g1, g2, g3, g4, g5, g6, g7,	\
 		  g8, g9, ga, gb, gc, gd, ge, gf },
 
+
+
 /*
  * GUID definitions of various offer types - services offered to the guest.
  */
@@ -1021,118 +1023,94 @@ int vmbus_allocate_mmio(struct resource **new, struct hv_device *device_obj,
  * {f8615163-df3e-46c5-913f-f2d2f965ed0e}
  */
 #define HV_NIC_GUID \
-	.guid = { \
-			0x63, 0x51, 0x61, 0xf8, 0x3e, 0xdf, 0xc5, 0x46, \
-			0x91, 0x3f, 0xf2, 0xd2, 0xf9, 0x65, 0xed, 0x0e \
-		}
+	.guid = UUID_LE(0xf8615163, 0xdf3e, 0x46c5, 0x91, 0x3f, \
+			0xf2, 0xd2, 0xf9, 0x65, 0xed, 0x0e)
 
 /*
  * IDE GUID
  * {32412632-86cb-44a2-9b5c-50d1417354f5}
  */
 #define HV_IDE_GUID \
-	.guid = { \
-			0x32, 0x26, 0x41, 0x32, 0xcb, 0x86, 0xa2, 0x44, \
-			0x9b, 0x5c, 0x50, 0xd1, 0x41, 0x73, 0x54, 0xf5 \
-		}
+	.guid = UUID_LE(0x32412632, 0x86cb, 0x44a2, 0x9b, 0x5c, \
+			0x50, 0xd1, 0x41, 0x73, 0x54, 0xf5)
 
 /*
  * SCSI GUID
  * {ba6163d9-04a1-4d29-b605-72e2ffb1dc7f}
  */
 #define HV_SCSI_GUID \
-	.guid = { \
-			0xd9, 0x63, 0x61, 0xba, 0xa1, 0x04, 0x29, 0x4d, \
-			0xb6, 0x05, 0x72, 0xe2, 0xff, 0xb1, 0xdc, 0x7f \
-		}
+	.guid = UUID_LE(0xba6163d9, 0x04a1, 0x4d29, 0xb6, 0x05, \
+			0x72, 0xe2, 0xff, 0xb1, 0xdc, 0x7f)
 
 /*
  * Shutdown GUID
  * {0e0b6031-5213-4934-818b-38d90ced39db}
  */
 #define HV_SHUTDOWN_GUID \
-	.guid = { \
-			0x31, 0x60, 0x0b, 0x0e, 0x13, 0x52, 0x34, 0x49, \
-			0x81, 0x8b, 0x38, 0xd9, 0x0c, 0xed, 0x39, 0xdb \
-		}
+	.guid = UUID_LE(0x0e0b6031, 0x5213, 0x4934, 0x81, 0x8b, \
+			0x38, 0xd9, 0x0c, 0xed, 0x39, 0xdb)
 
 /*
  * Time Synch GUID
  * {9527E630-D0AE-497b-ADCE-E80AB0175CAF}
  */
 #define HV_TS_GUID \
-	.guid = { \
-			0x30, 0xe6, 0x27, 0x95, 0xae, 0xd0, 0x7b, 0x49, \
-			0xad, 0xce, 0xe8, 0x0a, 0xb0, 0x17, 0x5c, 0xaf \
-		}
+	.guid = UUID_LE(0x9527e630, 0xd0ae, 0x497b, 0xad, 0xce, \
+			0xe8, 0x0a, 0xb0, 0x17, 0x5c, 0xaf)
 
 /*
  * Heartbeat GUID
  * {57164f39-9115-4e78-ab55-382f3bd5422d}
  */
 #define HV_HEART_BEAT_GUID \
-	.guid = { \
-			0x39, 0x4f, 0x16, 0x57, 0x15, 0x91, 0x78, 0x4e, \
-			0xab, 0x55, 0x38, 0x2f, 0x3b, 0xd5, 0x42, 0x2d \
-		}
+	.guid = UUID_LE(0x57164f39, 0x9115, 0x4e78, 0xab, 0x55, \
+			0x38, 0x2f, 0x3b, 0xd5, 0x42, 0x2d)
 
 /*
  * KVP GUID
  * {a9a0f4e7-5a45-4d96-b827-8a841e8c03e6}
  */
 #define HV_KVP_GUID \
-	.guid = { \
-			0xe7, 0xf4, 0xa0, 0xa9, 0x45, 0x5a, 0x96, 0x4d, \
-			0xb8, 0x27, 0x8a, 0x84, 0x1e, 0x8c, 0x3,  0xe6 \
-		}
+	.guid = UUID_LE(0xa9a0f4e7, 0x5a45, 0x4d96, 0xb8, 0x27, \
+			0x8a, 0x84, 0x1e, 0x8c, 0x03, 0xe6)
 
 /*
  * Dynamic memory GUID
  * {525074dc-8985-46e2-8057-a307dc18a502}
  */
 #define HV_DM_GUID \
-	.guid = { \
-			0xdc, 0x74, 0x50, 0X52, 0x85, 0x89, 0xe2, 0x46, \
-			0x80, 0x57, 0xa3, 0x07, 0xdc, 0x18, 0xa5, 0x02 \
-		}
+	.guid = UUID_LE(0x525074dc, 0x8985, 0x46e2, 0x80, 0x57, \
+			0xa3, 0x07, 0xdc, 0x18, 0xa5, 0x02)
 
 /*
  * Mouse GUID
  * {cfa8b69e-5b4a-4cc0-b98b-8ba1a1f3f95a}
  */
 #define HV_MOUSE_GUID \
-	.guid = { \
-			0x9e, 0xb6, 0xa8, 0xcf, 0x4a, 0x5b, 0xc0, 0x4c, \
-			0xb9, 0x8b, 0x8b, 0xa1, 0xa1, 0xf3, 0xf9, 0x5a \
-		}
+	.guid = UUID_LE(0xcfa8b69e, 0x5b4a, 0x4cc0, 0xb9, 0x8b, \
+			0x8b, 0xa1, 0xa1, 0xf3, 0xf9, 0x5a)
 
 /*
  * VSS (Backup/Restore) GUID
  */
 #define HV_VSS_GUID \
-	.guid = { \
-			0x29, 0x2e, 0xfa, 0x35, 0x23, 0xea, 0x36, 0x42, \
-			0x96, 0xae, 0x3a, 0x6e, 0xba, 0xcb, 0xa4,  0x40 \
-		}
+	.guid = UUID_LE(0x35fa2e29, 0xea23, 0x4236, 0x96, 0xae, \
+			0x3a, 0x6e, 0xba, 0xcb, 0xa4, 0x40)
 /*
  * Synthetic Video GUID
  * {DA0A7802-E377-4aac-8E77-0558EB1073F8}
  */
 #define HV_SYNTHVID_GUID \
-	.guid = { \
-			0x02, 0x78, 0x0a, 0xda, 0x77, 0xe3, 0xac, 0x4a, \
-			0x8e, 0x77, 0x05, 0x58, 0xeb, 0x10, 0x73, 0xf8 \
-		}
+	.guid = UUID_LE(0xda0a7802, 0xe377, 0x4aac, 0x8e, 0x77, \
+			0x05, 0x58, 0xeb, 0x10, 0x73, 0xf8)
 
 /*
  * Synthetic FC GUID
  * {2f9bcc4a-0069-4af3-b76b-6fd0be528cda}
  */
 #define HV_SYNTHFC_GUID \
-	.guid = { \
-			0x4A, 0xCC, 0x9B, 0x2F, 0x69, 0x00, 0xF3, 0x4A, \
-			0xB7, 0x6B, 0x6F, 0xD0, 0xBE, 0x52, 0x8C, 0xDA \
-		}
+	.guid = UUID_LE(0x2f9bcc4a, 0x0069, 0x4af3, 0xb7, 0x6b, \
+			0x6f, 0xd0, 0xbe, 0x52, 0x8c, 0xda)
 
 /*
  * Guest File Copy Service
@@ -1140,20 +1118,16 @@ int vmbus_allocate_mmio(struct resource **new, struct hv_device *device_obj,
  */
 
 #define HV_FCOPY_GUID \
-	.guid = { \
-			0xE3, 0x4B, 0xD1, 0x34, 0xE4, 0xDE, 0xC8, 0x41, \
-			0x9A, 0xE7, 0x6B, 0x17, 0x49, 0x77, 0xC1, 0x92 \
-		}
+	.guid = UUID_LE(0x34d14be3, 0xdee4, 0x41c8, 0x9a, 0xe7, \
+			0x6b, 0x17, 0x49, 0x77, 0xc1, 0x92)
 
 /*
  * NetworkDirect. This is the guest RDMA service.
  * {8c2eaf3d-32a7-4b09-ab99-bd1f1c86b501}
  */
 #define HV_ND_GUID \
-	.guid = { \
-			0x3d, 0xaf, 0x2e, 0x8c, 0xa7, 0x32, 0x09, 0x4b, \
-			0xab, 0x99, 0xbd, 0x1f, 0x1c, 0x86, 0xb5, 0x01 \
-		}
+	.guid = UUID_LE(0x8c2eaf3d, 0x32a7, 0x4b09, 0xab, 0x99, \
+			0xbd, 0x1f, 0x1c, 0x86, 0xb5, 0x01)
 
 /*
  * PCI Express Pass Through
@@ -1161,10 +1135,8 @@ int vmbus_allocate_mmio(struct resource **new, struct hv_device *device_obj,
  */
 
 #define HV_PCIE_GUID \
-	.guid = { \
-			0x1D, 0xF6, 0xC4, 0x44, 0x44, 0x44, 0x00, 0x44, \
-			0x9D, 0x52, 0x80, 0x2E, 0x27, 0xED, 0xE1, 0x9F \
-		}
+	.guid = UUID_LE(0x44c4f61d, 0x4444, 0x4400, 0x9d, 0x52, \
+			0x80, 0x2e, 0x27, 0xed, 0xe1, 0x9f)
 
 /*
  * Common header for Hyper-V ICs
diff --git a/include/linux/mod_devicetable.h b/include/linux/mod_devicetable.h
index 64f36e09a790..6e4c645e1c0d 100644
--- a/include/linux/mod_devicetable.h
+++ b/include/linux/mod_devicetable.h
@@ -404,7 +404,7 @@ struct virtio_device_id {
  * For Hyper-V devices we use the device guid as the id.
  */
 struct hv_vmbus_device_id {
-	__u8 guid[16];
+	uuid_le guid;
 	kernel_ulong_t driver_data;	/* Data private to the driver */
 };
 
diff --git a/scripts/mod/file2alias.c b/scripts/mod/file2alias.c
index 9f5cdd49ff0b..8e8c69bee78f 100644
--- a/scripts/mod/file2alias.c
+++ b/scripts/mod/file2alias.c
@@ -917,7 +917,7 @@ static int do_vmbus_entry(const char *filename, void *symval,
 	char guid_name[(sizeof(*guid) + 1) * 2];
 
 	for (i = 0; i < (sizeof(*guid) * 2); i += 2)
-		sprintf(&guid_name[i], "%02x", TO_NATIVE((*guid)[i/2]));
+		sprintf(&guid_name[i], "%02x", TO_NATIVE((guid->b)[i/2]));
 
 	strcpy(alias, "vmbus:");
 	strcat(alias, guid_name);
-- 
2.13.0

