From 389cac6ccf5d05e70ee37b0b4df0991aa7120966 Mon Sep 17 00:00:00 2001
From: "K. Y. Srinivasan" <kys@microsoft.com>
Date: Fri, 25 Dec 2015 20:00:30 -0800
Subject: [PATCH 25/44] Drivers: hv: vmbus: Add vendor and device atttributes

Add vendor and device attributes to VMBUS devices. These will be used
by Hyper-V tools as well user-level RDMA libraries that will use the
vendor/device tuple to discover the RDMA device.

Signed-off-by: K. Y. Srinivasan <kys@microsoft.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
(cherry picked from commit 7047f17d70fc0599563d30d0791692cb5fe42ae6)
---
 Documentation/ABI/stable/sysfs-bus-vmbus |  14 +++
 drivers/hv/channel_mgmt.c                | 166 +++++++++++++++++++++++--------
 drivers/hv/vmbus_drv.c                   |  21 ++++
 include/linux/hyperv.h                   |  28 ++++++
 4 files changed, 186 insertions(+), 43 deletions(-)

diff --git a/Documentation/ABI/stable/sysfs-bus-vmbus b/Documentation/ABI/stable/sysfs-bus-vmbus
index 636e938d5e33..5d0125f7bcaf 100644
--- a/Documentation/ABI/stable/sysfs-bus-vmbus
+++ b/Documentation/ABI/stable/sysfs-bus-vmbus
@@ -27,3 +27,17 @@ Description:	The mapping of which primary/sub channels are bound to which
 		Virtual Processors.
 		Format: <channel's child_relid:the bound cpu's number>
 Users:		tools/hv/lsvmbus
+
+What:		/sys/bus/vmbus/devices/vmbus_*/device
+Date:		Dec. 2015
+KernelVersion:	4.5
+Contact:	K. Y. Srinivasan <kys@microsoft.com>
+Description:	The 16 bit device ID of the device
+Users:		tools/hv/lsvmbus and user level RDMA libraries
+
+What:		/sys/bus/vmbus/devices/vmbus_*/vendor
+Date:		Dec. 2015
+KernelVersion:	4.5
+Contact:	K. Y. Srinivasan <kys@microsoft.com>
+Description:	The 16 bit vendor ID of the device
+Users:		tools/hv/lsvmbus and user level RDMA libraries
diff --git a/drivers/hv/channel_mgmt.c b/drivers/hv/channel_mgmt.c
index 763d0c19c16f..d6c611457601 100644
--- a/drivers/hv/channel_mgmt.c
+++ b/drivers/hv/channel_mgmt.c
@@ -33,8 +33,122 @@
 
 #include "hyperv_vmbus.h"
 
-static void init_vp_index(struct vmbus_channel *channel,
-			  const uuid_le *type_guid);
+static void init_vp_index(struct vmbus_channel *channel, u16 dev_type);
+
+static const struct vmbus_device vmbus_devs[] = {
+	/* IDE */
+	{ .dev_type = HV_IDE,
+	  HV_IDE_GUID,
+	  .perf_device = true,
+	},
+
+	/* SCSI */
+	{ .dev_type = HV_SCSI,
+	  HV_SCSI_GUID,
+	  .perf_device = true,
+	},
+
+	/* Fibre Channel */
+	{ .dev_type = HV_FC,
+	  HV_SYNTHFC_GUID,
+	  .perf_device = true,
+	},
+
+	/* Synthetic NIC */
+	{ .dev_type = HV_NIC,
+	  HV_NIC_GUID,
+	  .perf_device = true,
+	},
+
+	/* Network Direct */
+	{ .dev_type = HV_ND,
+	  HV_ND_GUID,
+	  .perf_device = true,
+	},
+
+	/* PCIE */
+	{ .dev_type = HV_PCIE,
+	  HV_PCIE_GUID,
+	  .perf_device = true,
+	},
+
+	/* Synthetic Frame Buffer */
+	{ .dev_type = HV_FB,
+	  HV_SYNTHVID_GUID,
+	  .perf_device = false,
+	},
+
+	/* Synthetic Keyboard */
+	{ .dev_type = HV_KBD,
+	  HV_KBD_GUID,
+	  .perf_device = false,
+	},
+
+	/* Synthetic MOUSE */
+	{ .dev_type = HV_MOUSE,
+	  HV_MOUSE_GUID,
+	  .perf_device = false,
+	},
+
+	/* KVP */
+	{ .dev_type = HV_KVP,
+	  HV_KVP_GUID,
+	  .perf_device = false,
+	},
+
+	/* Time Synch */
+	{ .dev_type = HV_TS,
+	  HV_TS_GUID,
+	  .perf_device = false,
+	},
+
+	/* Heartbeat */
+	{ .dev_type = HV_HB,
+	  HV_HEART_BEAT_GUID,
+	  .perf_device = false,
+	},
+
+	/* Shutdown */
+	{ .dev_type = HV_SHUTDOWN,
+	  HV_SHUTDOWN_GUID,
+	  .perf_device = false,
+	},
+
+	/* File copy */
+	{ .dev_type = HV_FCOPY,
+	  HV_FCOPY_GUID,
+	  .perf_device = false,
+	},
+
+	/* Backup */
+	{ .dev_type = HV_BACKUP,
+	  HV_VSS_GUID,
+	  .perf_device = false,
+	},
+
+	/* Dynamic Memory */
+	{ .dev_type = HV_DM,
+	  HV_DM_GUID,
+	  .perf_device = false,
+	},
+
+	/* Unknown GUID */
+	{ .dev_type = HV_UNKOWN,
+	  .perf_device = false,
+	},
+};
+
+static u16 hv_get_dev_type(const uuid_le *guid)
+{
+	u16 i;
+
+	for (i = HV_IDE; i < HV_UNKOWN; i++) {
+		if (!uuid_le_cmp(*guid, vmbus_devs[i].guid))
+			return i;
+	}
+	pr_info("Unknown GUID: %pUl\n", guid);
+	return i;
+}
 
 /**
  * vmbus_prep_negotiate_resp() - Create default response for Hyper-V Negotiate message
@@ -252,6 +366,7 @@ static void vmbus_process_offer(struct vmbus_channel *newchannel)
 	struct vmbus_channel *channel;
 	bool fnew = true;
 	unsigned long flags;
+	u16 dev_type;
 
 	/* Make sure this is a new offer */
 	mutex_lock(&vmbus_connection.channel_mutex);
@@ -289,7 +404,9 @@ static void vmbus_process_offer(struct vmbus_channel *newchannel)
 			goto err_free_chan;
 	}
 
-	init_vp_index(newchannel, &newchannel->offermsg.offer.if_type);
+	dev_type = hv_get_dev_type(&newchannel->offermsg.offer.if_type);
+
+	init_vp_index(newchannel, dev_type);
 
 	if (newchannel->target_cpu != get_cpu()) {
 		put_cpu();
@@ -326,6 +443,7 @@ static void vmbus_process_offer(struct vmbus_channel *newchannel)
 	if (!newchannel->device_obj)
 		goto err_deq_chan;
 
+	newchannel->device_obj->device_id = dev_type;
 	/*
 	 * Add the new device to the bus. This will kick off device-driver
 	 * binding which eventually invokes the device driver's AddDevice()
@@ -359,37 +477,6 @@ err_free_chan:
 	free_channel(newchannel);
 }
 
-enum {
-	IDE = 0,
-	SCSI,
-	FC,
-	NIC,
-	ND_NIC,
-	PCIE,
-	MAX_PERF_CHN,
-};
-
-/*
- * This is an array of device_ids (device types) that are performance critical.
- * We attempt to distribute the interrupt load for these devices across
- * all available CPUs.
- */
-static const struct hv_vmbus_device_id hp_devs[] = {
-	/* IDE */
-	{ HV_IDE_GUID, },
-	/* Storage - SCSI */
-	{ HV_SCSI_GUID, },
-	/* Storage - FC */
-	{ HV_SYNTHFC_GUID, },
-	/* Network */
-	{ HV_NIC_GUID, },
-	/* NetworkDirect Guest RDMA */
-	{ HV_ND_GUID, },
-	/* PCI Express Pass Through */
-	{ HV_PCIE_GUID, },
-};
-
-
 /*
  * We use this state to statically distribute the channel interrupt load.
  */
@@ -406,22 +493,15 @@ static int next_numa_node_id;
  * For pre-win8 hosts or non-performance critical channels we assign the
  * first CPU in the first NUMA node.
  */
-static void init_vp_index(struct vmbus_channel *channel, const uuid_le *type_guid)
+static void init_vp_index(struct vmbus_channel *channel, u16 dev_type)
 {
 	u32 cur_cpu;
-	int i;
-	bool perf_chn = false;
+	bool perf_chn = vmbus_devs[dev_type].perf_device;
 	struct vmbus_channel *primary = channel->primary_channel;
 	int next_node;
 	struct cpumask available_mask;
 	struct cpumask *alloced_mask;
 
-	for (i = IDE; i < MAX_PERF_CHN; i++) {
-		if (!uuid_le_cmp(*type_guid, hp_devs[i].guid)) {
-			perf_chn = true;
-			break;
-		}
-	}
 	if ((vmbus_proto_version == VERSION_WS2008) ||
 	    (vmbus_proto_version == VERSION_WIN7) || (!perf_chn)) {
 		/*
diff --git a/drivers/hv/vmbus_drv.c b/drivers/hv/vmbus_drv.c
index e71f3561dbab..f688c051ca17 100644
--- a/drivers/hv/vmbus_drv.c
+++ b/drivers/hv/vmbus_drv.c
@@ -480,6 +480,24 @@ static ssize_t channel_vp_mapping_show(struct device *dev,
 }
 static DEVICE_ATTR_RO(channel_vp_mapping);
 
+static ssize_t vendor_show(struct device *dev,
+			   struct device_attribute *dev_attr,
+			   char *buf)
+{
+	struct hv_device *hv_dev = device_to_hv_device(dev);
+	return sprintf(buf, "0x%x\n", hv_dev->vendor_id);
+}
+static DEVICE_ATTR_RO(vendor);
+
+static ssize_t device_show(struct device *dev,
+			   struct device_attribute *dev_attr,
+			   char *buf)
+{
+	struct hv_device *hv_dev = device_to_hv_device(dev);
+	return sprintf(buf, "0x%x\n", hv_dev->device_id);
+}
+static DEVICE_ATTR_RO(device);
+
 /* Set up per device attributes in /sys/bus/vmbus/devices/<bus device> */
 static struct attribute *vmbus_attrs[] = {
 	&dev_attr_id.attr,
@@ -505,6 +523,8 @@ static struct attribute *vmbus_attrs[] = {
 	&dev_attr_in_read_bytes_avail.attr,
 	&dev_attr_in_write_bytes_avail.attr,
 	&dev_attr_channel_vp_mapping.attr,
+	&dev_attr_vendor.attr,
+	&dev_attr_device.attr,
 	NULL,
 };
 ATTRIBUTE_GROUPS(vmbus);
@@ -963,6 +983,7 @@ struct hv_device *vmbus_device_create(const uuid_le *type,
 	memcpy(&child_device_obj->dev_type, type, sizeof(uuid_le));
 	memcpy(&child_device_obj->dev_instance, instance,
 	       sizeof(uuid_le));
+	child_device_obj->vendor_id = 0x1414; /* MSFT vendor ID */
 
 
 	return child_device_obj;
diff --git a/include/linux/hyperv.h b/include/linux/hyperv.h
index 9e2de6a7cc96..51c98fd6044d 100644
--- a/include/linux/hyperv.h
+++ b/include/linux/hyperv.h
@@ -635,6 +635,32 @@ enum hv_signal_policy {
 	HV_SIGNAL_POLICY_EXPLICIT,
 };
 
+enum vmbus_device_type {
+	HV_IDE = 0,
+	HV_SCSI,
+	HV_FC,
+	HV_NIC,
+	HV_ND,
+	HV_PCIE,
+	HV_FB,
+	HV_KBD,
+	HV_MOUSE,
+	HV_KVP,
+	HV_TS,
+	HV_HB,
+	HV_SHUTDOWN,
+	HV_FCOPY,
+	HV_BACKUP,
+	HV_DM,
+	HV_UNKOWN,
+};
+
+struct vmbus_device {
+	u16  dev_type;
+	uuid_le guid;
+	bool perf_device;
+};
+
 struct vmbus_channel {
 	/* Unique channel id */
 	int id;
@@ -961,6 +987,8 @@ struct hv_device {
 
 	/* the device instance id of this device */
 	uuid_le dev_instance;
+	u16 vendor_id;
+	u16 device_id;
 
 	struct device device;
 
-- 
2.13.0

