From 076de0d8086f75b10632476ad8f128095adde73c Mon Sep 17 00:00:00 2001
From: Stefan Hajnoczi <stefanha@redhat.com>
Date: Thu, 17 Dec 2015 16:53:43 +0800
Subject: [PATCH 01/41] virtio: make find_vqs() checkpatch.pl-friendly

checkpatch.pl wants arrays of strings declared as follows:

  static const char * const names[] = { "vq-1", "vq-2", "vq-3" };

Currently the find_vqs() function takes a const char *names[] argument
so passing checkpatch.pl's const char * const names[] results in a
compiler error due to losing the second const.

This patch adjusts the find_vqs() prototype and updates all virtio
transports.  This makes it possible for virtio_balloon.c, virtio_input.c,
virtgpu_kms.c, and virtio_rpmsg_bus.c to use the checkpatch.pl-friendly
type.

Signed-off-by: Stefan Hajnoczi <stefanha@redhat.com>
Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
Acked-by: Bjorn Andersson <bjorn.andersson@sonymobile.com>
(cherry picked from commit f7ad26ff952b3ca2702d7da03aad0ab1f6c01d7c)
---
 drivers/gpu/drm/virtio/virtgpu_kms.c   | 2 +-
 drivers/misc/mic/card/mic_virtio.c     | 2 +-
 drivers/remoteproc/remoteproc_virtio.c | 2 +-
 drivers/rpmsg/virtio_rpmsg_bus.c       | 2 +-
 drivers/s390/virtio/kvm_virtio.c       | 2 +-
 drivers/s390/virtio/virtio_ccw.c       | 2 +-
 drivers/virtio/virtio_balloon.c        | 2 +-
 drivers/virtio/virtio_input.c          | 2 +-
 drivers/virtio/virtio_mmio.c           | 2 +-
 drivers/virtio/virtio_pci_common.c     | 4 ++--
 drivers/virtio/virtio_pci_common.h     | 2 +-
 drivers/virtio/virtio_pci_modern.c     | 2 +-
 include/linux/virtio_config.h          | 2 +-
 13 files changed, 14 insertions(+), 14 deletions(-)

diff --git a/drivers/gpu/drm/virtio/virtgpu_kms.c b/drivers/gpu/drm/virtio/virtgpu_kms.c
index 06496a1..4150873 100644
--- a/drivers/gpu/drm/virtio/virtgpu_kms.c
+++ b/drivers/gpu/drm/virtio/virtgpu_kms.c
@@ -130,7 +130,7 @@ int virtio_gpu_driver_load(struct drm_device *dev, unsigned long flags)
 	static vq_callback_t *callbacks[] = {
 		virtio_gpu_ctrl_ack, virtio_gpu_cursor_ack
 	};
-	static const char *names[] = { "control", "cursor" };
+	static const char * const names[] = { "control", "cursor" };
 
 	struct virtio_gpu_device *vgdev;
 	/* this will expand later */
diff --git a/drivers/misc/mic/card/mic_virtio.c b/drivers/misc/mic/card/mic_virtio.c
index e486a0c..f6ed57d 100644
--- a/drivers/misc/mic/card/mic_virtio.c
+++ b/drivers/misc/mic/card/mic_virtio.c
@@ -311,7 +311,7 @@ unmap:
 static int mic_find_vqs(struct virtio_device *vdev, unsigned nvqs,
 			struct virtqueue *vqs[],
 			vq_callback_t *callbacks[],
-			const char *names[])
+			const char * const names[])
 {
 	struct mic_vdev *mvdev = to_micvdev(vdev);
 	struct mic_device_ctrl __iomem *dc = mvdev->dc;
diff --git a/drivers/remoteproc/remoteproc_virtio.c b/drivers/remoteproc/remoteproc_virtio.c
index e1a1023..e44872f 100644
--- a/drivers/remoteproc/remoteproc_virtio.c
+++ b/drivers/remoteproc/remoteproc_virtio.c
@@ -147,7 +147,7 @@ static void rproc_virtio_del_vqs(struct virtio_device *vdev)
 static int rproc_virtio_find_vqs(struct virtio_device *vdev, unsigned nvqs,
 		       struct virtqueue *vqs[],
 		       vq_callback_t *callbacks[],
-		       const char *names[])
+		       const char * const names[])
 {
 	struct rproc *rproc = vdev_to_rproc(vdev);
 	int i, ret;
diff --git a/drivers/rpmsg/virtio_rpmsg_bus.c b/drivers/rpmsg/virtio_rpmsg_bus.c
index 73354ee..1fcd27c 100644
--- a/drivers/rpmsg/virtio_rpmsg_bus.c
+++ b/drivers/rpmsg/virtio_rpmsg_bus.c
@@ -945,7 +945,7 @@ static void rpmsg_ns_cb(struct rpmsg_channel *rpdev, void *data, int len,
 static int rpmsg_probe(struct virtio_device *vdev)
 {
 	vq_callback_t *vq_cbs[] = { rpmsg_recv_done, rpmsg_xmit_done };
-	const char *names[] = { "input", "output" };
+	static const char * const names[] = { "input", "output" };
 	struct virtqueue *vqs[2];
 	struct virtproc_info *vrp;
 	void *bufs_va;
diff --git a/drivers/s390/virtio/kvm_virtio.c b/drivers/s390/virtio/kvm_virtio.c
index 53fb975..1d060fd 100644
--- a/drivers/s390/virtio/kvm_virtio.c
+++ b/drivers/s390/virtio/kvm_virtio.c
@@ -255,7 +255,7 @@ static void kvm_del_vqs(struct virtio_device *vdev)
 static int kvm_find_vqs(struct virtio_device *vdev, unsigned nvqs,
 			struct virtqueue *vqs[],
 			vq_callback_t *callbacks[],
-			const char *names[])
+			const char * const names[])
 {
 	struct kvm_device *kdev = to_kvmdev(vdev);
 	int i;
diff --git a/drivers/s390/virtio/virtio_ccw.c b/drivers/s390/virtio/virtio_ccw.c
index 1b83159..bf2d130 100644
--- a/drivers/s390/virtio/virtio_ccw.c
+++ b/drivers/s390/virtio/virtio_ccw.c
@@ -635,7 +635,7 @@ out:
 static int virtio_ccw_find_vqs(struct virtio_device *vdev, unsigned nvqs,
 			       struct virtqueue *vqs[],
 			       vq_callback_t *callbacks[],
-			       const char *names[])
+			       const char * const names[])
 {
 	struct virtio_ccw_device *vcdev = to_vc_device(vdev);
 	unsigned long *indicatorp = NULL;
diff --git a/drivers/virtio/virtio_balloon.c b/drivers/virtio/virtio_balloon.c
index 7d3e5d0..0c3691f 100644
--- a/drivers/virtio/virtio_balloon.c
+++ b/drivers/virtio/virtio_balloon.c
@@ -388,7 +388,7 @@ static int init_vqs(struct virtio_balloon *vb)
 {
 	struct virtqueue *vqs[3];
 	vq_callback_t *callbacks[] = { balloon_ack, balloon_ack, stats_request };
-	const char *names[] = { "inflate", "deflate", "stats" };
+	static const char * const names[] = { "inflate", "deflate", "stats" };
 	int err, nvqs;
 
 	/*
diff --git a/drivers/virtio/virtio_input.c b/drivers/virtio/virtio_input.c
index c96944b..350a2a5 100644
--- a/drivers/virtio/virtio_input.c
+++ b/drivers/virtio/virtio_input.c
@@ -170,7 +170,7 @@ static int virtinput_init_vqs(struct virtio_input *vi)
 	struct virtqueue *vqs[2];
 	vq_callback_t *cbs[] = { virtinput_recv_events,
 				 virtinput_recv_status };
-	static const char *names[] = { "events", "status" };
+	static const char * const names[] = { "events", "status" };
 	int err;
 
 	err = vi->vdev->config->find_vqs(vi->vdev, 2, vqs, cbs, names);
diff --git a/drivers/virtio/virtio_mmio.c b/drivers/virtio/virtio_mmio.c
index f499d9d..745c6ee 100644
--- a/drivers/virtio/virtio_mmio.c
+++ b/drivers/virtio/virtio_mmio.c
@@ -482,7 +482,7 @@ error_available:
 static int vm_find_vqs(struct virtio_device *vdev, unsigned nvqs,
 		       struct virtqueue *vqs[],
 		       vq_callback_t *callbacks[],
-		       const char *names[])
+		       const char * const names[])
 {
 	struct virtio_mmio_device *vm_dev = to_virtio_mmio_device(vdev);
 	unsigned int irq = platform_get_irq(vm_dev->pdev, 0);
diff --git a/drivers/virtio/virtio_pci_common.c b/drivers/virtio/virtio_pci_common.c
index 2046a68..f6bed86 100644
--- a/drivers/virtio/virtio_pci_common.c
+++ b/drivers/virtio/virtio_pci_common.c
@@ -296,7 +296,7 @@ void vp_del_vqs(struct virtio_device *vdev)
 static int vp_try_to_find_vqs(struct virtio_device *vdev, unsigned nvqs,
 			      struct virtqueue *vqs[],
 			      vq_callback_t *callbacks[],
-			      const char *names[],
+			      const char * const names[],
 			      bool use_msix,
 			      bool per_vq_vectors)
 {
@@ -376,7 +376,7 @@ error_find:
 int vp_find_vqs(struct virtio_device *vdev, unsigned nvqs,
 		struct virtqueue *vqs[],
 		vq_callback_t *callbacks[],
-		const char *names[])
+		const char * const names[])
 {
 	int err;
 
diff --git a/drivers/virtio/virtio_pci_common.h b/drivers/virtio/virtio_pci_common.h
index b976d96..2cc2522 100644
--- a/drivers/virtio/virtio_pci_common.h
+++ b/drivers/virtio/virtio_pci_common.h
@@ -139,7 +139,7 @@ void vp_del_vqs(struct virtio_device *vdev);
 int vp_find_vqs(struct virtio_device *vdev, unsigned nvqs,
 		       struct virtqueue *vqs[],
 		       vq_callback_t *callbacks[],
-		       const char *names[]);
+		       const char * const names[]);
 const char *vp_bus_name(struct virtio_device *vdev);
 
 /* Setup the affinity for a virtqueue:
diff --git a/drivers/virtio/virtio_pci_modern.c b/drivers/virtio/virtio_pci_modern.c
index 4469202..631021c 100644
--- a/drivers/virtio/virtio_pci_modern.c
+++ b/drivers/virtio/virtio_pci_modern.c
@@ -423,7 +423,7 @@ err_new_queue:
 static int vp_modern_find_vqs(struct virtio_device *vdev, unsigned nvqs,
 			      struct virtqueue *vqs[],
 			      vq_callback_t *callbacks[],
-			      const char *names[])
+			      const char * const names[])
 {
 	struct virtio_pci_device *vp_dev = to_vp_device(vdev);
 	struct virtqueue *vq;
diff --git a/include/linux/virtio_config.h b/include/linux/virtio_config.h
index e5ce8ab..6e6cb0c 100644
--- a/include/linux/virtio_config.h
+++ b/include/linux/virtio_config.h
@@ -70,7 +70,7 @@ struct virtio_config_ops {
 	int (*find_vqs)(struct virtio_device *, unsigned nvqs,
 			struct virtqueue *vqs[],
 			vq_callback_t *callbacks[],
-			const char *names[]);
+			const char * const names[]);
 	void (*del_vqs)(struct virtio_device *);
 	u64 (*get_features)(struct virtio_device *vdev);
 	int (*finalize_features)(struct virtio_device *vdev);
-- 
2.8.2

