From 454e636edd0bb26495afb3850a37aa5e5214a4ed Mon Sep 17 00:00:00 2001
From: Thomas Gleixner <tglx@linutronix.de>
Date: Mon, 18 Jul 2011 17:10:12 +0200
Subject: [PATCH 051/283] mips: Disable highmem on RT

The current highmem handling on -RT is not compatible and needs fixups.

Signed-off-by: Thomas Gleixner <tglx@linutronix.de>
---
 arch/mips/Kconfig | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/mips/Kconfig b/arch/mips/Kconfig
index 201caf226b47..bd268302efa4 100644
--- a/arch/mips/Kconfig
+++ b/arch/mips/Kconfig
@@ -2517,7 +2517,7 @@ config MIPS_CRC_SUPPORT
 #
 config HIGHMEM
 	bool "High Memory Support"
-	depends on 32BIT && CPU_SUPPORTS_HIGHMEM && SYS_SUPPORTS_HIGHMEM && !CPU_MIPS32_3_5_EVA
+	depends on 32BIT && CPU_SUPPORTS_HIGHMEM && SYS_SUPPORTS_HIGHMEM && !CPU_MIPS32_3_5_EVA && !PREEMPT_RT_FULL
 
 config CPU_SUPPORTS_HIGHMEM
 	bool
-- 
2.20.1

