From ba73d346b0dd3efc44de486866fca2daa1959026 Mon Sep 17 00:00:00 2001
From: Cathy Avery <cavery@redhat.com>
Date: Tue, 31 Oct 2017 08:52:06 -0400
Subject: [PATCH 20/21] scsi: storvsc: Allow only one remove lun work item to
 be issued per lun

When running multipath on a VM if all available paths go down the driver
can schedule large amounts of storvsc_remove_lun work items to the same
lun. In response to the failing paths typically storvsc responds by
taking host->scan_mutex and issuing a TUR per lun. If there has been
heavy IO to the failed device all the failed IOs are returned from the
host. A remove lun work item is issued per failed IO. If the outstanding
TURs have not been completed in a timely manner the scan_mutex is never
released or released too late. Consequently the many remove lun work
items are not completed as scsi_remove_device also tries to take
host->scan_mutex.  This results in dragging the VM down and sometimes
completely.

This patch only allows one remove lun to be issued to a particular lun
while it is an instantiated member of the scsi stack.

Signed-off-by: Cathy Avery <cavery@redhat.com>
Reviewed-by: Christoph Hellwig <hch@lst.de>
Reviewed-by: Long Li <longli@microsoft.com>
Signed-off-by: Martin K. Petersen <martin.petersen@oracle.com>
(cherry picked from commit 436ad941335386c5fc7faa915a8fbdfe8c908084)
---
 drivers/scsi/storvsc_drv.c | 27 ++++++++++++++++++++++-----
 1 file changed, 22 insertions(+), 5 deletions(-)

diff --git a/drivers/scsi/storvsc_drv.c b/drivers/scsi/storvsc_drv.c
index 5adeb1e4b186..405b5da45fa1 100644
--- a/drivers/scsi/storvsc_drv.c
+++ b/drivers/scsi/storvsc_drv.c
@@ -486,6 +486,7 @@ struct hv_host_device {
 	unsigned int port;
 	unsigned char path;
 	unsigned char target;
+	struct workqueue_struct *handle_error_wq;
 };
 
 struct storvsc_scan_work {
@@ -931,6 +932,7 @@ static void storvsc_handle_error(struct vmscsi_request *vm_srb,
 {
 	struct storvsc_scan_work *wrk;
 	void (*process_err_fn)(struct work_struct *work);
+	struct hv_host_device *host_dev = shost_priv(host);
 	bool do_work = false;
 
 	switch (SRB_STATUS(vm_srb->srb_status)) {
@@ -998,7 +1000,7 @@ static void storvsc_handle_error(struct vmscsi_request *vm_srb,
 	wrk->lun = vm_srb->lun;
 	wrk->tgt_id = vm_srb->target_id;
 	INIT_WORK(&wrk->work, process_err_fn);
-	schedule_work(&wrk->work);
+	queue_work(host_dev->handle_error_wq, &wrk->work);
 }
 
 
@@ -1816,10 +1818,19 @@ static int storvsc_probe(struct hv_device *device,
 	if (stor_device->num_sc != 0)
 		host->nr_hw_queues = stor_device->num_sc + 1;
 
+	/*
+	 * Set the error handler work queue.
+	 */
+	host_dev->handle_error_wq =
+			alloc_ordered_workqueue("storvsc_error_wq_%d",
+						WQ_MEM_RECLAIM,
+						host->host_no);
+	if (!host_dev->handle_error_wq)
+		goto err_out2;
 	/* Register the HBA and start the scsi bus scan */
 	ret = scsi_add_host(host, &device->device);
 	if (ret != 0)
-		goto err_out2;
+		goto err_out3;
 
 	if (!dev_is_ide) {
 		scsi_scan_host(host);
@@ -1828,7 +1839,7 @@ static int storvsc_probe(struct hv_device *device,
 			 device->dev_instance.b[4]);
 		ret = scsi_add_device(host, 0, target, 0);
 		if (ret)
-			goto err_out3;
+			goto err_out4;
 	}
 #if IS_ENABLED(CONFIG_SCSI_FC_ATTRS)
 	if (host->transportt == fc_transport_template) {
@@ -1839,17 +1850,21 @@ static int storvsc_probe(struct hv_device *device,
 		fc_host_node_name(host) = stor_device->node_name;
 		fc_host_port_name(host) = stor_device->port_name;
 		stor_device->rport = fc_remote_port_add(host, 0, &ids);
+
 		if (!stor_device->rport) {
 			ret = -ENOMEM;
-			goto err_out3;
+			goto err_out4;
 		}
 	}
 #endif
 	return 0;
 
-err_out3:
+err_out4:
 	scsi_remove_host(host);
 
+err_out3:
+	destroy_workqueue(host_dev->handle_error_wq);
+
 err_out2:
 	/*
 	 * Once we have connected with the host, we would need to
@@ -1873,6 +1888,7 @@ static int storvsc_remove(struct hv_device *dev)
 {
 	struct storvsc_device *stor_device = hv_get_drvdata(dev);
 	struct Scsi_Host *host = stor_device->host;
+	struct hv_host_device *host_dev = shost_priv(host);
 
 #if IS_ENABLED(CONFIG_SCSI_FC_ATTRS)
 	if (host->transportt == fc_transport_template) {
@@ -1880,6 +1896,7 @@ static int storvsc_remove(struct hv_device *dev)
 		fc_remove_host(host);
 	}
 #endif
+	destroy_workqueue(host_dev->handle_error_wq);
 	scsi_remove_host(host);
 	storvsc_dev_remove(dev);
 	scsi_host_put(host);
-- 
2.24.0

