From 297ef639cbc4bc3aac2e5a8835090136753796fc Mon Sep 17 00:00:00 2001
From: Thomas Gleixner <tglx@linutronix.de>
Date: Tue, 14 Jul 2015 14:26:34 +0200
Subject: [PATCH 048/283] powerpc: Use generic rwsem on RT

Use generic code which uses rtmutex

Signed-off-by: Thomas Gleixner <tglx@linutronix.de>
---
 arch/powerpc/Kconfig | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

diff --git a/arch/powerpc/Kconfig b/arch/powerpc/Kconfig
index a80669209155..9952764db9c5 100644
--- a/arch/powerpc/Kconfig
+++ b/arch/powerpc/Kconfig
@@ -105,10 +105,11 @@ config LOCKDEP_SUPPORT
 
 config RWSEM_GENERIC_SPINLOCK
 	bool
+	default y if PREEMPT_RT_FULL
 
 config RWSEM_XCHGADD_ALGORITHM
 	bool
-	default y
+	default y if !PREEMPT_RT_FULL
 
 config GENERIC_LOCKBREAK
 	bool
-- 
2.20.1

