From af21e5c755447f232fe96ab7df9ecaf8df8a15a7 Mon Sep 17 00:00:00 2001
From: Sebastian Andrzej Siewior <bigeasy@linutronix.de>
Date: Thu, 19 May 2016 17:45:27 +0200
Subject: [PATCH 208/283] kernel/printk: Don't try to print from IRQ/NMI region

On -RT we try to acquire sleeping locks which might lead to warnings
from lockdep or a warn_on() from spin_try_lock() (which is a rtmutex on
RT).
We don't print in general from a IRQ off region so we should not try
this via console_unblank() / bust_spinlocks() as well.

Signed-off-by: Sebastian Andrzej Siewior <bigeasy@linutronix.de>
---
 kernel/printk/printk.c | 10 ++++++++++
 1 file changed, 10 insertions(+)

diff --git a/kernel/printk/printk.c b/kernel/printk/printk.c
index d983c509f74a..f15988a33860 100644
--- a/kernel/printk/printk.c
+++ b/kernel/printk/printk.c
@@ -1782,6 +1782,11 @@ static void call_console_drivers(const char *ext_text, size_t ext_len,
 	if (!console_drivers)
 		return;
 
+	if (IS_ENABLED(CONFIG_PREEMPT_RT_BASE)) {
+		if (in_irq() || in_nmi())
+			return;
+	}
+
 	migrate_disable();
 	for_each_console(con) {
 		if (exclusive_console && con != exclusive_console)
@@ -2540,6 +2545,11 @@ void console_unblank(void)
 {
 	struct console *c;
 
+	if (IS_ENABLED(CONFIG_PREEMPT_RT_BASE)) {
+		if (in_irq() || in_nmi())
+			return;
+	}
+
 	/*
 	 * console_unblank can no longer be called in interrupt context unless
 	 * oops_in_progress is set to 1..
-- 
2.20.1

