From 13e8b97c81d4029a2c41ce13ffc84507af252845 Mon Sep 17 00:00:00 2001
From: Alexandre Belloni <alexandre.belloni@bootlin.com>
Date: Thu, 13 Sep 2018 13:30:19 +0200
Subject: [PATCH 002/283] clocksource/drivers: Add a new driver for the Atmel
 ARM TC blocks

Add a driver for the Atmel Timer Counter Blocks. This driver provides a
clocksource and two clockevent devices.

One of the clockevent device is linked to the clocksource counter and so it
will run at the same frequency. This will be used when there is only on TCB
channel available for timers.

The other clockevent device runs on a separate TCB channel when available.

This driver uses regmap and syscon to be able to probe early in the boot
and avoid having to switch on the TCB clocksource later. Using regmap also
means that unused TCB channels may be used by other drivers (PWM for
example). read/writel are still used to access channel specific registers
to avoid the performance impact of regmap (mainly locking).

Tested-by: Alexander Dahl <ada@thorsis.com>
Tested-by: Andras Szemzo <szemzo.andras@gmail.com>
Signed-off-by: Alexandre Belloni <alexandre.belloni@bootlin.com>
Signed-off-by: Sebastian Andrzej Siewior <bigeasy@linutronix.de>
---
 drivers/clocksource/Kconfig           |   8 +
 drivers/clocksource/Makefile          |   3 +-
 drivers/clocksource/timer-atmel-tcb.c | 410 ++++++++++++++++++++++++++
 3 files changed, 420 insertions(+), 1 deletion(-)
 create mode 100644 drivers/clocksource/timer-atmel-tcb.c

diff --git a/drivers/clocksource/Kconfig b/drivers/clocksource/Kconfig
index 4d37f018d846..0ab22e7037f4 100644
--- a/drivers/clocksource/Kconfig
+++ b/drivers/clocksource/Kconfig
@@ -415,6 +415,14 @@ config ATMEL_ST
 	help
 	  Support for the Atmel ST timer.
 
+config ATMEL_ARM_TCB_CLKSRC
+	bool "Microchip ARM TC Block" if COMPILE_TEST
+	select REGMAP_MMIO
+	depends on GENERIC_CLOCKEVENTS
+	help
+	  This enables build of clocksource and clockevent driver for
+	  the integrated Timer Counter Blocks in Microchip ARM SoCs.
+
 config CLKSRC_EXYNOS_MCT
 	bool "Exynos multi core timer driver" if COMPILE_TEST
 	depends on ARM || ARM64
diff --git a/drivers/clocksource/Makefile b/drivers/clocksource/Makefile
index db51b2427e8a..0df9384a1230 100644
--- a/drivers/clocksource/Makefile
+++ b/drivers/clocksource/Makefile
@@ -3,7 +3,8 @@ obj-$(CONFIG_TIMER_OF)		+= timer-of.o
 obj-$(CONFIG_TIMER_PROBE)	+= timer-probe.o
 obj-$(CONFIG_ATMEL_PIT)		+= timer-atmel-pit.o
 obj-$(CONFIG_ATMEL_ST)		+= timer-atmel-st.o
-obj-$(CONFIG_ATMEL_TCB_CLKSRC)	+= tcb_clksrc.o
+obj-$(CONFIG_ATMEL_TCB_CLKSRC) += tcb_clksrc.o
+obj-$(CONFIG_ATMEL_ARM_TCB_CLKSRC)	+= timer-atmel-tcb.o
 obj-$(CONFIG_X86_PM_TIMER)	+= acpi_pm.o
 obj-$(CONFIG_SCx200HR_TIMER)	+= scx200_hrt.o
 obj-$(CONFIG_CS5535_CLOCK_EVENT_SRC)	+= cs5535-clockevt.o
diff --git a/drivers/clocksource/timer-atmel-tcb.c b/drivers/clocksource/timer-atmel-tcb.c
new file mode 100644
index 000000000000..21fbe430f91b
--- /dev/null
+++ b/drivers/clocksource/timer-atmel-tcb.c
@@ -0,0 +1,410 @@
+// SPDX-License-Identifier: GPL-2.0
+#include <linux/clk.h>
+#include <linux/clockchips.h>
+#include <linux/clocksource.h>
+#include <linux/interrupt.h>
+#include <linux/kernel.h>
+#include <linux/mfd/syscon.h>
+#include <linux/of_address.h>
+#include <linux/of_irq.h>
+#include <linux/regmap.h>
+#include <linux/sched_clock.h>
+#include <soc/at91/atmel_tcb.h>
+
+struct atmel_tcb_clksrc {
+	struct clocksource clksrc;
+	struct clock_event_device clkevt;
+	struct regmap *regmap;
+	void __iomem *base;
+	struct clk *clk[2];
+	char name[20];
+	int channels[2];
+	int bits;
+	int irq;
+	struct {
+		u32 cmr;
+		u32 imr;
+		u32 rc;
+		bool clken;
+	} cache[2];
+	u32 bmr_cache;
+	bool registered;
+	bool clk_enabled;
+};
+
+static struct atmel_tcb_clksrc tc;
+
+static struct clk *tcb_clk_get(struct device_node *node, int channel)
+{
+	struct clk *clk;
+	char clk_name[] = "t0_clk";
+
+	clk_name[1] += channel;
+	clk = of_clk_get_by_name(node->parent, clk_name);
+	if (!IS_ERR(clk))
+		return clk;
+
+	return of_clk_get_by_name(node->parent, "t0_clk");
+}
+
+/*
+ * Clocksource and clockevent using the same channel(s)
+ */
+static u64 tc_get_cycles(struct clocksource *cs)
+{
+	u32 lower, upper;
+
+	do {
+		upper = readl_relaxed(tc.base + ATMEL_TC_CV(tc.channels[1]));
+		lower = readl_relaxed(tc.base + ATMEL_TC_CV(tc.channels[0]));
+	} while (upper != readl_relaxed(tc.base + ATMEL_TC_CV(tc.channels[1])));
+
+	return (upper << 16) | lower;
+}
+
+static u64 tc_get_cycles32(struct clocksource *cs)
+{
+	return readl_relaxed(tc.base + ATMEL_TC_CV(tc.channels[0]));
+}
+
+static u64 notrace tc_sched_clock_read(void)
+{
+	return tc_get_cycles(&tc.clksrc);
+}
+
+static u64 notrace tc_sched_clock_read32(void)
+{
+	return tc_get_cycles32(&tc.clksrc);
+}
+
+static int tcb_clkevt_next_event(unsigned long delta,
+				 struct clock_event_device *d)
+{
+	u32 old, next, cur;
+
+	old = readl(tc.base + ATMEL_TC_CV(tc.channels[0]));
+	next = old + delta;
+	writel(next, tc.base + ATMEL_TC_RC(tc.channels[0]));
+	cur = readl(tc.base + ATMEL_TC_CV(tc.channels[0]));
+
+	/* check whether the delta elapsed while setting the register */
+	if ((next < old && cur < old && cur > next) ||
+	    (next > old && (cur < old || cur > next))) {
+		/*
+		 * Clear the CPCS bit in the status register to avoid
+		 * generating a spurious interrupt next time a valid
+		 * timer event is configured.
+		 */
+		old = readl(tc.base + ATMEL_TC_SR(tc.channels[0]));
+		return -ETIME;
+	}
+
+	writel(ATMEL_TC_CPCS, tc.base + ATMEL_TC_IER(tc.channels[0]));
+
+	return 0;
+}
+
+static irqreturn_t tc_clkevt_irq(int irq, void *handle)
+{
+	unsigned int sr;
+
+	sr = readl(tc.base + ATMEL_TC_SR(tc.channels[0]));
+	if (sr & ATMEL_TC_CPCS) {
+		tc.clkevt.event_handler(&tc.clkevt);
+		return IRQ_HANDLED;
+	}
+
+	return IRQ_NONE;
+}
+
+static int tcb_clkevt_oneshot(struct clock_event_device *dev)
+{
+	if (clockevent_state_oneshot(dev))
+		return 0;
+
+	/*
+	 * Because both clockevent devices may share the same IRQ, we don't want
+	 * the less likely one to stay requested
+	 */
+	return request_irq(tc.irq, tc_clkevt_irq, IRQF_TIMER | IRQF_SHARED,
+			   tc.name, &tc);
+}
+
+static int tcb_clkevt_shutdown(struct clock_event_device *dev)
+{
+	writel(0xff, tc.base + ATMEL_TC_IDR(tc.channels[0]));
+	if (tc.bits == 16)
+		writel(0xff, tc.base + ATMEL_TC_IDR(tc.channels[1]));
+
+	if (!clockevent_state_detached(dev))
+		free_irq(tc.irq, &tc);
+
+	return 0;
+}
+
+static void __init tcb_setup_dual_chan(struct atmel_tcb_clksrc *tc,
+				       int mck_divisor_idx)
+{
+	/* first channel: waveform mode, input mclk/8, clock TIOA on overflow */
+	writel(mck_divisor_idx			/* likely divide-by-8 */
+	       | ATMEL_TC_CMR_WAVE
+	       | ATMEL_TC_CMR_WAVESEL_UP	/* free-run */
+	       | ATMEL_TC_CMR_ACPA(SET)		/* TIOA rises at 0 */
+	       | ATMEL_TC_CMR_ACPC(CLEAR),	/* (duty cycle 50%) */
+	       tc->base + ATMEL_TC_CMR(tc->channels[0]));
+	writel(0x0000, tc->base + ATMEL_TC_RA(tc->channels[0]));
+	writel(0x8000, tc->base + ATMEL_TC_RC(tc->channels[0]));
+	writel(0xff, tc->base + ATMEL_TC_IDR(tc->channels[0]));	/* no irqs */
+	writel(ATMEL_TC_CCR_CLKEN, tc->base + ATMEL_TC_CCR(tc->channels[0]));
+
+	/* second channel: waveform mode, input TIOA */
+	writel(ATMEL_TC_CMR_XC(tc->channels[1])		/* input: TIOA */
+	       | ATMEL_TC_CMR_WAVE
+	       | ATMEL_TC_CMR_WAVESEL_UP,		/* free-run */
+	       tc->base + ATMEL_TC_CMR(tc->channels[1]));
+	writel(0xff, tc->base + ATMEL_TC_IDR(tc->channels[1]));	/* no irqs */
+	writel(ATMEL_TC_CCR_CLKEN, tc->base + ATMEL_TC_CCR(tc->channels[1]));
+
+	/* chain both channel, we assume the previous channel */
+	regmap_write(tc->regmap, ATMEL_TC_BMR,
+		     ATMEL_TC_BMR_TCXC(1 + tc->channels[1], tc->channels[1]));
+	/* then reset all the timers */
+	regmap_write(tc->regmap, ATMEL_TC_BCR, ATMEL_TC_BCR_SYNC);
+}
+
+static void __init tcb_setup_single_chan(struct atmel_tcb_clksrc *tc,
+					 int mck_divisor_idx)
+{
+	/* channel 0:  waveform mode, input mclk/8 */
+	writel(mck_divisor_idx			/* likely divide-by-8 */
+	       | ATMEL_TC_CMR_WAVE
+	       | ATMEL_TC_CMR_WAVESEL_UP,	/* free-run */
+	       tc->base + ATMEL_TC_CMR(tc->channels[0]));
+	writel(0xff, tc->base + ATMEL_TC_IDR(tc->channels[0]));	/* no irqs */
+	writel(ATMEL_TC_CCR_CLKEN, tc->base + ATMEL_TC_CCR(tc->channels[0]));
+
+	/* then reset all the timers */
+	regmap_write(tc->regmap, ATMEL_TC_BCR, ATMEL_TC_BCR_SYNC);
+}
+
+static void tc_clksrc_suspend(struct clocksource *cs)
+{
+	int i;
+
+	for (i = 0; i < 1 + (tc.bits == 16); i++) {
+		tc.cache[i].cmr = readl(tc.base + ATMEL_TC_CMR(tc.channels[i]));
+		tc.cache[i].imr = readl(tc.base + ATMEL_TC_IMR(tc.channels[i]));
+		tc.cache[i].rc = readl(tc.base + ATMEL_TC_RC(tc.channels[i]));
+		tc.cache[i].clken = !!(readl(tc.base +
+					     ATMEL_TC_SR(tc.channels[i])) &
+				       ATMEL_TC_CLKSTA);
+	}
+
+	if (tc.bits == 16)
+		regmap_read(tc.regmap, ATMEL_TC_BMR, &tc.bmr_cache);
+}
+
+static void tc_clksrc_resume(struct clocksource *cs)
+{
+	int i;
+
+	for (i = 0; i < 1 + (tc.bits == 16); i++) {
+		/* Restore registers for the channel, RA and RB are not used  */
+		writel(tc.cache[i].cmr, tc.base + ATMEL_TC_CMR(tc.channels[i]));
+		writel(tc.cache[i].rc, tc.base + ATMEL_TC_RC(tc.channels[i]));
+		writel(0, tc.base + ATMEL_TC_RA(tc.channels[i]));
+		writel(0, tc.base + ATMEL_TC_RB(tc.channels[i]));
+		/* Disable all the interrupts */
+		writel(0xff, tc.base + ATMEL_TC_IDR(tc.channels[i]));
+		/* Reenable interrupts that were enabled before suspending */
+		writel(tc.cache[i].imr, tc.base + ATMEL_TC_IER(tc.channels[i]));
+
+		/* Start the clock if it was used */
+		if (tc.cache[i].clken)
+			writel(ATMEL_TC_CCR_CLKEN, tc.base +
+			       ATMEL_TC_CCR(tc.channels[i]));
+	}
+
+	/* in case of dual channel, chain channels */
+	if (tc.bits == 16)
+		regmap_write(tc.regmap, ATMEL_TC_BMR, tc.bmr_cache);
+	/* Finally, trigger all the channels*/
+	regmap_write(tc.regmap, ATMEL_TC_BCR, ATMEL_TC_BCR_SYNC);
+}
+
+static int __init tcb_clksrc_register(struct device_node *node,
+				      struct regmap *regmap, void __iomem *base,
+				      int channel, int channel1, int irq,
+				      int bits)
+{
+	u32 rate, divided_rate = 0;
+	int best_divisor_idx = -1;
+	int i, err = -1;
+	u64 (*tc_sched_clock)(void);
+
+	tc.regmap = regmap;
+	tc.base = base;
+	tc.channels[0] = channel;
+	tc.channels[1] = channel1;
+	tc.irq = irq;
+	tc.bits = bits;
+
+	tc.clk[0] = tcb_clk_get(node, tc.channels[0]);
+	if (IS_ERR(tc.clk[0]))
+		return PTR_ERR(tc.clk[0]);
+	err = clk_prepare_enable(tc.clk[0]);
+	if (err) {
+		pr_debug("can't enable T0 clk\n");
+		goto err_clk;
+	}
+
+	/* How fast will we be counting?  Pick something over 5 MHz.  */
+	rate = (u32)clk_get_rate(tc.clk[0]);
+	for (i = 0; i < 5; i++) {
+		unsigned int divisor = atmel_tc_divisors[i];
+		unsigned int tmp;
+
+		if (!divisor)
+			continue;
+
+		tmp = rate / divisor;
+		pr_debug("TC: %u / %-3u [%d] --> %u\n", rate, divisor, i, tmp);
+		if (best_divisor_idx > 0) {
+			if (tmp < 5 * 1000 * 1000)
+				continue;
+		}
+		divided_rate = tmp;
+		best_divisor_idx = i;
+	}
+
+	if (tc.bits == 32) {
+		tc.clksrc.read = tc_get_cycles32;
+		tcb_setup_single_chan(&tc, best_divisor_idx);
+		tc_sched_clock = tc_sched_clock_read32;
+		snprintf(tc.name, sizeof(tc.name), "%s:%d",
+			 kbasename(node->parent->full_name), tc.channels[0]);
+	} else {
+		tc.clk[1] = tcb_clk_get(node, tc.channels[1]);
+		if (IS_ERR(tc.clk[1]))
+			goto err_disable_t0;
+
+		err = clk_prepare_enable(tc.clk[1]);
+		if (err) {
+			pr_debug("can't enable T1 clk\n");
+			goto err_clk1;
+		}
+		tc.clksrc.read = tc_get_cycles,
+		tcb_setup_dual_chan(&tc, best_divisor_idx);
+		tc_sched_clock = tc_sched_clock_read;
+		snprintf(tc.name, sizeof(tc.name), "%s:%d,%d",
+			 kbasename(node->parent->full_name), tc.channels[0],
+			 tc.channels[1]);
+	}
+
+	pr_debug("%s at %d.%03d MHz\n", tc.name,
+		 divided_rate / 1000000,
+		 ((divided_rate + 500000) % 1000000) / 1000);
+
+	tc.clksrc.name = tc.name;
+	tc.clksrc.suspend = tc_clksrc_suspend;
+	tc.clksrc.resume = tc_clksrc_resume;
+	tc.clksrc.rating = 200;
+	tc.clksrc.mask = CLOCKSOURCE_MASK(32);
+	tc.clksrc.flags = CLOCK_SOURCE_IS_CONTINUOUS;
+
+	err = clocksource_register_hz(&tc.clksrc, divided_rate);
+	if (err)
+		goto err_disable_t1;
+
+	sched_clock_register(tc_sched_clock, 32, divided_rate);
+
+	tc.registered = true;
+
+	/* Set up and register clockevents */
+	tc.clkevt.name = tc.name;
+	tc.clkevt.cpumask = cpumask_of(0);
+	tc.clkevt.set_next_event = tcb_clkevt_next_event;
+	tc.clkevt.set_state_oneshot = tcb_clkevt_oneshot;
+	tc.clkevt.set_state_shutdown = tcb_clkevt_shutdown;
+	tc.clkevt.features = CLOCK_EVT_FEAT_ONESHOT;
+	tc.clkevt.rating = 125;
+
+	clockevents_config_and_register(&tc.clkevt, divided_rate, 1,
+					BIT(tc.bits) - 1);
+
+	return 0;
+
+err_disable_t1:
+	if (tc.bits == 16)
+		clk_disable_unprepare(tc.clk[1]);
+
+err_clk1:
+	if (tc.bits == 16)
+		clk_put(tc.clk[1]);
+
+err_disable_t0:
+	clk_disable_unprepare(tc.clk[0]);
+
+err_clk:
+	clk_put(tc.clk[0]);
+
+	pr_err("%s: unable to register clocksource/clockevent\n",
+	       tc.clksrc.name);
+
+	return err;
+}
+
+static int __init tcb_clksrc_init(struct device_node *node)
+{
+	const struct of_device_id *match;
+	struct regmap *regmap;
+	void __iomem *tcb_base;
+	u32 channel;
+	int irq, err, chan1 = -1;
+	unsigned bits;
+
+	if (tc.registered)
+		return -ENODEV;
+
+	/*
+	 * The regmap has to be used to access registers that are shared
+	 * between channels on the same TCB but we keep direct IO access for
+	 * the counters to avoid the impact on performance
+	 */
+	regmap = syscon_node_to_regmap(node->parent);
+	if (IS_ERR(regmap))
+		return PTR_ERR(regmap);
+
+	tcb_base = of_iomap(node->parent, 0);
+	if (!tcb_base) {
+		pr_err("%s +%d %s\n", __FILE__, __LINE__, __func__);
+		return -ENXIO;
+	}
+
+	match = of_match_node(atmel_tcb_dt_ids, node->parent);
+	bits = (uintptr_t)match->data;
+
+	err = of_property_read_u32_index(node, "reg", 0, &channel);
+	if (err)
+		return err;
+
+	irq = of_irq_get(node->parent, channel);
+	if (irq < 0) {
+		irq = of_irq_get(node->parent, 0);
+		if (irq < 0)
+			return irq;
+	}
+
+	if (bits == 16) {
+		of_property_read_u32_index(node, "reg", 1, &chan1);
+		if (chan1 == -1) {
+			pr_err("%s: clocksource needs two channels\n",
+			       node->parent->full_name);
+			return -EINVAL;
+		}
+	}
+
+	return tcb_clksrc_register(node, regmap, tcb_base, channel, chan1, irq,
+				   bits);
+}
+TIMER_OF_DECLARE(atmel_tcb_clksrc, "atmel,tcb-timer", tcb_clksrc_init);
-- 
2.20.1

