From a3a039471f58abf91d2007ede9a7e308c834b456 Mon Sep 17 00:00:00 2001
From: Josh Cartwright <joshc@ni.com>
Date: Thu, 11 Feb 2016 11:54:01 -0600
Subject: [PATCH 212/283] KVM: arm/arm64: downgrade preempt_disable()d region
 to migrate_disable()

kvm_arch_vcpu_ioctl_run() disables the use of preemption when updating
the vgic and timer states to prevent the calling task from migrating to
another CPU.  It does so to prevent the task from writing to the
incorrect per-CPU GIC distributor registers.

On -rt kernels, it's possible to maintain the same guarantee with the
use of migrate_{disable,enable}(), with the added benefit that the
migrate-disabled region is preemptible.  Update
kvm_arch_vcpu_ioctl_run() to do so.

Cc: Christoffer Dall <christoffer.dall@linaro.org>
Reported-by: Manish Jaggi <Manish.Jaggi@caviumnetworks.com>
Signed-off-by: Josh Cartwright <joshc@ni.com>
Signed-off-by: Sebastian Andrzej Siewior <bigeasy@linutronix.de>
---
 virt/kvm/arm/arm.c | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

diff --git a/virt/kvm/arm/arm.c b/virt/kvm/arm/arm.c
index 02bac8abd206..d36802fe2825 100644
--- a/virt/kvm/arm/arm.c
+++ b/virt/kvm/arm/arm.c
@@ -712,7 +712,7 @@ int kvm_arch_vcpu_ioctl_run(struct kvm_vcpu *vcpu, struct kvm_run *run)
 		 * involves poking the GIC, which must be done in a
 		 * non-preemptible context.
 		 */
-		preempt_disable();
+		migrate_disable();
 
 		kvm_pmu_flush_hwstate(vcpu);
 
@@ -761,7 +761,7 @@ int kvm_arch_vcpu_ioctl_run(struct kvm_vcpu *vcpu, struct kvm_run *run)
 				kvm_timer_sync_hwstate(vcpu);
 			kvm_vgic_sync_hwstate(vcpu);
 			local_irq_enable();
-			preempt_enable();
+			migrate_enable();
 			continue;
 		}
 
@@ -839,7 +839,7 @@ int kvm_arch_vcpu_ioctl_run(struct kvm_vcpu *vcpu, struct kvm_run *run)
 		/* Exit types that need handling before we can be preempted */
 		handle_exit_early(vcpu, run, ret);
 
-		preempt_enable();
+		migrate_enable();
 
 		ret = handle_exit(vcpu, run, ret);
 	}
-- 
2.20.1

