From a4c6efd8adfd48a378c579bb7bc2c1a3162ced7f Mon Sep 17 00:00:00 2001
From: Sebastian Andrzej Siewior <bigeasy@linutronix.de>
Date: Wed, 26 Jun 2019 17:44:27 +0200
Subject: [PATCH 279/283] Revert "futex: workaround migrate_disable/enable in
 different context"

[ Upstream commit a71221d81cc4873891ae44f3aa02df596079b786 ]

Drop the RT fixup, the futex code will be changed to avoid the need for
the workaround.

Signed-off-by: Sebastian Andrzej Siewior <bigeasy@linutronix.de>
Signed-off-by: Steven Rostedt (VMware) <rostedt@goodmis.org>
---
 kernel/futex.c | 19 -------------------
 1 file changed, 19 deletions(-)

diff --git a/kernel/futex.c b/kernel/futex.c
index 1d9423914bf4..54ffc25183ed 100644
--- a/kernel/futex.c
+++ b/kernel/futex.c
@@ -2875,14 +2875,6 @@ static int futex_lock_pi(u32 __user *uaddr, unsigned int flags,
 	 * before __rt_mutex_start_proxy_lock() is done.
 	 */
 	raw_spin_lock_irq(&q.pi_state->pi_mutex.wait_lock);
-	/*
-	 * the migrate_disable() here disables migration in the in_atomic() fast
-	 * path which is enabled again in the following spin_unlock(). We have
-	 * one migrate_disable() pending in the slow-path which is reversed
-	 * after the raw_spin_unlock_irq() where we leave the atomic context.
-	 */
-	migrate_disable();
-
 	spin_unlock(q.lock_ptr);
 	/*
 	 * __rt_mutex_start_proxy_lock() unconditionally enqueues the @rt_waiter
@@ -2891,7 +2883,6 @@ static int futex_lock_pi(u32 __user *uaddr, unsigned int flags,
 	 */
 	ret = __rt_mutex_start_proxy_lock(&q.pi_state->pi_mutex, &rt_waiter, current);
 	raw_spin_unlock_irq(&q.pi_state->pi_mutex.wait_lock);
-	migrate_enable();
 
 	if (ret) {
 		if (ret == 1)
@@ -3040,21 +3031,11 @@ static int futex_unlock_pi(u32 __user *uaddr, unsigned int flags)
 		 * rt_waiter. Also see the WARN in wake_futex_pi().
 		 */
 		raw_spin_lock_irq(&pi_state->pi_mutex.wait_lock);
-		/*
-		 * Magic trickery for now to make the RT migrate disable
-		 * logic happy. The following spin_unlock() happens with
-		 * interrupts disabled so the internal migrate_enable()
-		 * won't undo the migrate_disable() which was issued when
-		 * locking hb->lock.
-		 */
-		migrate_disable();
 		spin_unlock(&hb->lock);
 
 		/* drops pi_state->pi_mutex.wait_lock */
 		ret = wake_futex_pi(uaddr, uval, pi_state);
 
-		migrate_enable();
-
 		put_pi_state(pi_state);
 
 		/*
-- 
2.20.1

