From 41661998f27ab61e9b5a134375ecb8c007c57c11 Mon Sep 17 00:00:00 2001
From: Xin Long <lucien.xin@gmail.com>
Date: Tue, 25 Apr 2017 22:58:37 +0800
Subject: [PATCH 14/14] bridge: move bridge multicast cleanup to ndo_uninit

During removing a bridge device, if the bridge is still up, a new mdb entry
still can be added in br_multicast_add_group() after all mdb entries are
removed in br_multicast_dev_del(). Like the path:

  mld_ifc_timer_expire ->
    mld_sendpack -> ...
      br_multicast_rcv ->
        br_multicast_add_group

The new mp's timer will be set up. If the timer expires after the bridge
is freed, it may cause use-after-free panic in br_multicast_group_expired.

BUG: unable to handle kernel NULL pointer dereference at 0000000000000048
IP: [<ffffffffa07ed2c8>] br_multicast_group_expired+0x28/0xb0 [bridge]
Call Trace:
 <IRQ>
 [<ffffffff81094536>] call_timer_fn+0x36/0x110
 [<ffffffffa07ed2a0>] ? br_mdb_free+0x30/0x30 [bridge]
 [<ffffffff81096967>] run_timer_softirq+0x237/0x340
 [<ffffffff8108dcbf>] __do_softirq+0xef/0x280
 [<ffffffff8169889c>] call_softirq+0x1c/0x30
 [<ffffffff8102c275>] do_softirq+0x65/0xa0
 [<ffffffff8108e055>] irq_exit+0x115/0x120
 [<ffffffff81699515>] smp_apic_timer_interrupt+0x45/0x60
 [<ffffffff81697a5d>] apic_timer_interrupt+0x6d/0x80

Nikolay also found it would cause a memory leak - the mdb hash is
reallocated and not freed due to the mdb rehash.

unreferenced object 0xffff8800540ba800 (size 2048):
  backtrace:
    [<ffffffff816e2287>] kmemleak_alloc+0x67/0xc0
    [<ffffffff81260bea>] __kmalloc+0x1ba/0x3e0
    [<ffffffffa05c60ee>] br_mdb_rehash+0x5e/0x340 [bridge]
    [<ffffffffa05c74af>] br_multicast_new_group+0x43f/0x6e0 [bridge]
    [<ffffffffa05c7aa3>] br_multicast_add_group+0x203/0x260 [bridge]
    [<ffffffffa05ca4b5>] br_multicast_rcv+0x945/0x11d0 [bridge]
    [<ffffffffa05b6b10>] br_dev_xmit+0x180/0x470 [bridge]
    [<ffffffff815c781b>] dev_hard_start_xmit+0xbb/0x3d0
    [<ffffffff815c8743>] __dev_queue_xmit+0xb13/0xc10
    [<ffffffff815c8850>] dev_queue_xmit+0x10/0x20
    [<ffffffffa02f8d7a>] ip6_finish_output2+0x5ca/0xac0 [ipv6]
    [<ffffffffa02fbfc6>] ip6_finish_output+0x126/0x2c0 [ipv6]
    [<ffffffffa02fc245>] ip6_output+0xe5/0x390 [ipv6]
    [<ffffffffa032b92c>] NF_HOOK.constprop.44+0x6c/0x240 [ipv6]
    [<ffffffffa032bd16>] mld_sendpack+0x216/0x3e0 [ipv6]
    [<ffffffffa032d5eb>] mld_ifc_timer_expire+0x18b/0x2b0 [ipv6]

This could happen when ip link remove a bridge or destroy a netns with a
bridge device inside.

With Nikolay's suggestion, this patch is to clean up bridge multicast in
ndo_uninit after bridge dev is shutdown, instead of br_dev_delete, so
that netif_running check in br_multicast_add_group can avoid this issue.

v1->v2:
  - fix this issue by moving br_multicast_dev_del to ndo_uninit, instead
    of calling dev_close in br_dev_delete.

(NOTE: Depends upon b6fe0440c637 ("bridge: implement missing ndo_uninit()"))

(NOTE: Manually fixed cherry-pick conflict as the code in the vicinity had
changed. The logic of this fix should be preserved)

Fixes: e10177abf842 ("bridge: multicast: fix handling of temp and perm entries")
Reported-by: Jianwen Ji <jiji@redhat.com>
Signed-off-by: Xin Long <lucien.xin@gmail.com>
Reviewed-by: Stephen Hemminger <stephen@networkplumber.org>
Signed-off-by: Nikolay Aleksandrov <nikolay@cumulusnetworks.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
Signed-off-by: Rolf Neugebauer <rn@rneugeba.io>
(cherry picked from commit b1b9d366028ff580e6dd80b48a69c473361456f1)
---
 net/bridge/br_device.c | 1 +
 net/bridge/br_if.c     | 1 -
 2 files changed, 1 insertion(+), 1 deletion(-)

diff --git a/net/bridge/br_device.c b/net/bridge/br_device.c
index 15be72678bc8..a0a7bb6a991f 100644
--- a/net/bridge/br_device.c
+++ b/net/bridge/br_device.c
@@ -126,6 +126,7 @@ static void br_dev_uninit(struct net_device *dev)
 {
 	struct net_bridge *br = netdev_priv(dev);
 
+	br_multicast_dev_del(br);
 	br_multicast_uninit_stats(br);
 	br_vlan_flush(br);
 	free_percpu(br->stats);
diff --git a/net/bridge/br_if.c b/net/bridge/br_if.c
index 191b1f23c160..93d08d1b039e 100644
--- a/net/bridge/br_if.c
+++ b/net/bridge/br_if.c
@@ -311,7 +311,6 @@ void br_dev_delete(struct net_device *dev, struct list_head *head)
 
 	br_fdb_delete_by_port(br, NULL, 0, 1);
 
-	br_multicast_dev_del(br);
 	del_timer_sync(&br->gc_timer);
 
 	br_sysfs_delbr(br->dev);
-- 
2.24.0

