From a6c38f0b349a8921a1bfe4dcef5972cf1e2224a0 Mon Sep 17 00:00:00 2001
From: Thomas Gleixner <tglx@linutronix.de>
Date: Fri, 3 Jul 2009 08:44:34 -0500
Subject: [PATCH 063/283] mm/scatterlist: Do not disable irqs on RT

For -RT it is enough to keep pagefault disabled (which is currently handled by
kmap_atomic()).

Signed-off-by: Thomas Gleixner <tglx@linutronix.de>
---
 lib/scatterlist.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/lib/scatterlist.c b/lib/scatterlist.c
index 7c6096a71704..5c2c68962709 100644
--- a/lib/scatterlist.c
+++ b/lib/scatterlist.c
@@ -776,7 +776,7 @@ void sg_miter_stop(struct sg_mapping_iter *miter)
 			flush_kernel_dcache_page(miter->page);
 
 		if (miter->__flags & SG_MITER_ATOMIC) {
-			WARN_ON_ONCE(preemptible());
+			WARN_ON_ONCE(!pagefault_disabled());
 			kunmap_atomic(miter->addr);
 		} else
 			kunmap(miter->page);
-- 
2.20.1

