# do not edit this file, it will be overwritten on update

# Alcatel One Touch X220D
# Alcatel One Touch X200
#
# These values were scraped from the X220D's Windows .inf files.  jrdmdm.inf
# lists the actual command and data (ie PPP) ports, while jrdser.inf lists the
# aux ports that may be either AT-capable or not but cannot be used for PPP.


ACTION!="add|change|move", GOTO="mm_x22x_port_types_end"
SUBSYSTEM!="tty", GOTO="mm_x22x_port_types_end"

SUBSYSTEMS=="usb", ATTRS{idVendor}=="1bbb", GOTO="mm_x22x_generic_vendorcheck"
SUBSYSTEMS=="usb", ATTRS{idVendor}=="0b3c", GOTO="mm_x22x_olivetti_vendorcheck"
GOTO="mm_x22x_port_types_end"

# Generic JRD devices ---------------------------

LABEL="mm_x22x_generic_vendorcheck"
SUBSYSTEMS=="usb", ATTRS{bInterfaceNumber}=="?*", ENV{.MM_USBIFNUM}="$attr{bInterfaceNumber}"

# Alcatel X200
ATTRS{idVendor}=="1bbb", ATTRS{idProduct}=="0000", ENV{.MM_USBIFNUM}=="03", ENV{ID_MM_X22X_PORT_TYPE_MODEM}="1"
ATTRS{idVendor}=="1bbb", ATTRS{idProduct}=="0000", ENV{.MM_USBIFNUM}=="00", ENV{ID_MM_X22X_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="1bbb", ATTRS{idProduct}=="0000", ENV{.MM_USBIFNUM}=="01", ENV{ID_MM_X22X_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="1bbb", ATTRS{idProduct}=="0000", ENV{.MM_USBIFNUM}=="02", ENV{ID_MM_X22X_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="1bbb", ATTRS{idProduct}=="0000", ENV{ID_MM_X22X_TAGGED}="1"

ATTRS{idVendor}=="1bbb", ATTRS{idProduct}=="0017", ENV{.MM_USBIFNUM}=="05", ENV{ID_MM_X22X_PORT_TYPE_MODEM}="1"
ATTRS{idVendor}=="1bbb", ATTRS{idProduct}=="0017", ENV{.MM_USBIFNUM}=="00", ENV{ID_MM_X22X_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="1bbb", ATTRS{idProduct}=="0017", ENV{.MM_USBIFNUM}=="01", ENV{ID_MM_X22X_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="1bbb", ATTRS{idProduct}=="0017", ENV{.MM_USBIFNUM}=="02", ENV{ID_MM_X22X_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="1bbb", ATTRS{idProduct}=="0017", ENV{.MM_USBIFNUM}=="03", ENV{ID_MM_X22X_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="1bbb", ATTRS{idProduct}=="0017", ENV{ID_MM_X22X_TAGGED}="1"

# Archos G9
ATTRS{idVendor}=="1bbb", ATTRS{idProduct}=="00B7", ENV{.MM_USBIFNUM}=="04", ENV{ID_MM_X22X_PORT_TYPE_MODEM}="1"
ATTRS{idVendor}=="1bbb", ATTRS{idProduct}=="00B7", ENV{.MM_USBIFNUM}=="00", ENV{ID_MM_X22X_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="1bbb", ATTRS{idProduct}=="00B7", ENV{.MM_USBIFNUM}=="01", ENV{ID_MM_X22X_PORT_TYPE_NMEA}="1"
ATTRS{idVendor}=="1bbb", ATTRS{idProduct}=="00B7", ENV{.MM_USBIFNUM}=="02", ENV{ID_MM_X22X_PORT_TYPE_VOICE}="1"
ATTRS{idVendor}=="1bbb", ATTRS{idProduct}=="00B7", ENV{.MM_USBIFNUM}=="03", ENV{ID_MM_X22X_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="1bbb", ATTRS{idProduct}=="00B7", ENV{ID_MM_X22X_TAGGED}="1"

GOTO="mm_x22x_port_types_end"

# Olivetti devices ---------------------------

LABEL="mm_x22x_olivetti_vendorcheck"
SUBSYSTEMS=="usb", ATTRS{bInterfaceNumber}=="?*", ENV{.MM_USBIFNUM}="$attr{bInterfaceNumber}"

# Olicard 200
ATTRS{idVendor}=="0b3c", ATTRS{idProduct}=="c005", ENV{.MM_USBIFNUM}=="05", ENV{ID_MM_X22X_PORT_TYPE_MODEM}="1"
ATTRS{idVendor}=="0b3c", ATTRS{idProduct}=="c005", ENV{.MM_USBIFNUM}=="00", ENV{ID_MM_X22X_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="0b3c", ATTRS{idProduct}=="c005", ENV{.MM_USBIFNUM}=="01", ENV{ID_MM_X22X_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="0b3c", ATTRS{idProduct}=="c005", ENV{.MM_USBIFNUM}=="02", ENV{ID_MM_X22X_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="0b3c", ATTRS{idProduct}=="c005", ENV{.MM_USBIFNUM}=="03", ENV{ID_MM_X22X_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="0b3c", ATTRS{idProduct}=="c005", ENV{.MM_USBIFNUM}=="06", ENV{ID_MM_X22X_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="0b3c", ATTRS{idProduct}=="c005", ENV{ID_MM_X22X_TAGGED}="1"

GOTO="mm_x22x_port_types_end"

LABEL="mm_x22x_port_types_end"
